Moore’s Law predicting development of chip, which number of transitions per silicon chip doubles every year.

This law breaking down because engineers are unable to develop chips with smaller transistors, as well as the limitation of size of an atomic.